#Raspberry Pi

![Raspberry Pi](./images/rpi.jpg)

##Geek的盛宴

Raspberry Pi是一款针对电脑业余爱好者、教师、小学生以及小型企业等用户的迷你电脑，预装Linux系统，体积仅信用卡大小，搭载ARM架构处理器，运算性能和智能手机相仿。在接口方面，Raspberry Pi提供了可供键鼠使用的USB接口，此外还有千兆以太网接口、SD卡扩展接口以及1个HDMI高清视频输出接口，可与显示器或者TV相连。

Linux是一套免费使用和自由传播的类Unix操作系统，是一个基于POSIX和UNIX的多用户、多任务、支持多线程和多CPU的操作系统。它能运行主要的UNIX工具软件、应用程序和网络协议。它支持32位和64位硬件。Linux继承了Unix以网络为核心的设计思想，是一个性能稳定的多用户网络操作系统。

Raspberry Pi相比于一般的ARM开发板来说，由于其本身搭载着Linux操作系统，可以用诸如Python、Ruby或Bash来执行脚本，而不是通过编译程序来运行，具有更高的开发效率。

##Raspberry Pi 初始化

今天的Raspberry Pi默认已经安装``openssh-server``，并已经可以登陆上去了。


接着我们就可以看到系统启动了，要我们输入用户名和密码

```bash
Raspbian GNU/Linux 7 raspberrypi ttyAMA0

raspberrypi login: pi
Password:
Last login: Sat Apr 26 05:58:07 UTC 2014 on ttyAMA0
Linux raspberrypi 3.10.25+ #622 PREEMPT Fri Jan 3 18:41:00 GMT 2014 armv6l

The programs included with the Debian GNU/Linux system are free software;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/*/copyright.

Debian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
permitted by applicable law.
ls

NOTICE: the software on this Raspberry Pi has not been fully configured. Please run 'sudo raspi-config'
```

然后

```bash
sudo raspi-config
```

选择第一个，下面就可以继续了
 
 ```
Expand Filesystem              Ensures that all of the SD card s
```

##Raspberry Pi GPIO

![GPIO](./images/gpio.png)

##Raspberry Pi


